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	Item No:
	VT-1864

	SKU Codes
	4228:3000K

	Base
	E27

	Real Watts
	12W

	EQ. Watts
	75W

	Voltage
	100~240V

	Input Frequency
	50/60Hz

	Input Current
	72ma

	Input Efficiency
	87lm/w

	Lumen(lm)
	1055lm/w

	PF
	>0.5

	CRI
	>80

	Color Temperature
	3000K,4500K,6000K

	Beam Angle
	200’D

	LED Chip
	SMD 2835

	LED Qty
	27

	Driver
	Constant current non-isolated driver

	Protection Class
	IP20

	Body Material
	Plastic

	Dimmable
	No

	Unit size
	60mmx118mm

	[bookmark: _GoBack]Life Time
	20000hrs

	Operation Temperature
	-25 ~50’C

	Applicable Environment
	[bookmark: OLE_LINK3][bookmark: OLE_LINK4]Indoor Lighting, Used in Home down light, Stairwell lighting.
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Color Temperature:2700KColor Temperature:4000K
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Color Temperature:6500K


Instruction Manual：
Installing please following below steps:
1. Please note to cut off the power supply before replacing the lamp to prevent electric shock or lamp burning, choose to install to correspondingly lampholders
2. When try to tighten or take off the bulb, please clench radiator body by finger as shown below :
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3. When need to take off the bulb ,please wait 20minutes after turning off,so as not to burn your fingers
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